For 1990-2009 cars

Figure 1: |

(1) | Coolant Surge Tank
(2) | Engine Wiring Harness
(3) | Torque Axis Mount
(4) | Low Coolant Sensor Connector
(5) | A/C Transducer Connector (LD9)
(6) | A/C Pipe Assembly
(7) | Canister Vent Solenoid

Figure 2: |

#### Generator Harness Routing (LD9)

(1) | MAP Sensor
(2) | Engine Harness to Bracket Clips
(3) | Canister Purge Solenoid
(4) | A/C Compressor Connector
(5) | A/C Compressor
(6) | Generator
(7) | IAC Sensor

Figure 3: |

#### LD9

(1) | Crankshaft Sensor
(2) | Intake Manifold Bracket
(3) | Engine Wiring Harness to Intake Manifold Bracket
(4) | A/C Compressor Connector

Figure 4: |

#### LD9

(1) | CAM Position Connector Sensor
(2) | EGR Solenoid
(3) | Injector Connector #4
(4) | T.P.S. Sensor Connector
(5) | Injector Connector #3
(6) | Injector Connector #2
(7) | Injector Connector #1

Figure 5: |

#### Engine Harness Ground (LD9)

(1) | Engine Grounds Lead
(2) | Fan Lead
(3) | Engine Harness to Stud Clip
(4) | Engine Stud
(5) | Cooling Fan Lead

Figure 6: |

#### Starter Harness Routing (L82)

(1) | Engine Wiring Harness
(2) | Oil Pressure Sensor
(3) | Starter Motor Assembly
(4) | Detonation Sensor
(5) | Oil Pan
(6) | A/C Compressor Clutch Connection
(7) | A/C Compressor
(8) | Water Pump
(9) | Crank Sensor Inter Connection

Figure 7: |

#### 3100 L82

(1) | Engine Wiring Ground Leads
(2) | ABS Wheel Sensor Leads
(3) | Engine Wiring Harness
(4) | Cooling Fan Lead

Figure 8: |

#### Front of Engine (3100 L82)

Figure 9: |

#### 3100 L82

(1) | ABS Wheel Sensor Lead
(2) | Main Engine Wiring Harness
(3) | MAF Sensor Connector
(4) | MAT Sensor Connector
(5) | IAC Connector
(6) | EGR Solenoid Connector
(7) | TPS Connector
(8) | Cooling Fan Lead
(9) | TCC Connector