For 1990-2009 cars

### Removal Procedure

The fuel pump relay is mounted in the right front corner of the engine compartment.

1. Turn the ignition OFF.
2. Remove the fuel pump relay from mounting bracket.
3. Remove the fuel pump relay from the fuel pump relay electrical connector.

### Installation Procedure

1. Install the fuel pump relay.
2. Install the fuel pump relay electrical connector.
3. Turn the ignition ON.