For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION:The clutch release bearing is noisy with the clutch fully engaged.
1 | Check the clutch release bearing for binding on the transmission bearing retainer. Is the clutch release bearing binding on the transmission bearing retainer? | -- | Go to Step 2 | --
2 | Clean and lubricate the affected area. Replace the clutch actuator cylinder if necessary. Refer to Clutch Actuator Cylinder Replacement . Is the clutch release bearing still noisy? | -- | -- | System OK