For 1990-2009 cars

# SQUEALING NOISE COMING FROM FRONT BRAKES

#### SUBJECT: SQUEALING NOISE COMING FROM FRONT BRAKES (INSTALL NEW BRAKE PADS)

#### MODELS: 1997 CHEVROLET MALIBU 1997 OLDSMOBILE CUTLASS

#### CONDITION:

SOME OWNERS MAY COMMENT ON A SQUEALING NOISE COMING FROM THE FRONT BRAKES.

#### CORRECTION:

REPLACE THE FRONT DISC BRAKE PADS, P/N 18026184. REFER TO SECTION 5B1 IN THE SERVICE MANUAL. REVISED PADS HAVE AN ENHANCED NOISE INSULATOR MATERIAL ON THE BACK OF EACH BRAKE PAD.

#### IMPORTANT:

DO NOT RESURFACE BRAKE ROTORS. REPLACE BRAKE ROTORS IF THERE IS A PULSATION CONCERN.

#### IMPORTANT:

EVERY BRAKE SERVICE SHOULD INCLUDE CLEANING AND LUBING ALL METAL TO METAL CONTACT POINTS (I.E.; CALIPER TO KNUCKLE, PAD TO KNUCKLE, ETC.). ALSO, CORRECT CLEARANCES MUST BE CHECKED.

#### PARTS INFORMATION:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: H0042 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.