For 1990-2009 cars

#### Tools Required

• | J 6125-1B Slide Hammer

• | J 23129 Converter Housing Seal Remover

1. Assemble J 6125-1B and J 23129 .

Important: Do not damage the transmission case during the removal of the torque converter seal assembly.

2. Remove the oil seal assembly (525) from the case:

• | Use J 6125-1B and J 23129 in order to remove the seal

• | Install J 23129 between the seal and stator support

• | Alternately, use a large, flat blade screwdriver in order to pry out the seal. Use a block of wood to pry against