For 1990-2009 cars

Table 1: | A/C Compressor Clutch Relay
Table 2: | Ignition Switch C1
Table 3: | Ignition Switch C2

#### A/C Compressor Clutch Relay

Connector Part Information |

• | 12129716

• | 4-Way F Metri-Pack Series 280 FLX LK (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | PNK | 439 | Fuse Output-Ignition-1
85 | DK GRN/ WHT | 459 | Air Conditioning Control Relay Output-Coil
86 | PNK | 439 | Vehicle Speed Signal
87 | DK GRN | 59 | Air Conditioning Compressor Clutch Feed

#### Ignition Switch C1

Connector Part Information |

• | 12129842

• | 6-Way F Metri-Pack Series 280, 630

(NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 3 | Ignition Switch Output - Ignition 1
B | ORN | 300 | Ignition Switch Output - Ignition 3
C | YEL | 5 | Ignition Switch Output - Crank
D | WHT | 1390 | Ignition Switch Output - Off, Run, Crank
E | BLK | 150 | Ground
F | BLK | 150 | Ground

#### Ignition Switch C2

Connector Part Information |

• | 12162229

• | 6-Way F Metri-Pack Series 280, 630

(BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 4 | Ignition Switch Output - Accessory
B | RED | 242 | Fuse Output - Battery - Type II Fuse
C | RED | 242 | Fuse Output - Battery - Type II Fuse
D | BLK | 1350 | Ground
E | -- | -- | Not Used
F | GRN LT | 80 | Key Reminder Switch Signal