For 1990-2009 cars

Table 1: | A/C Compressor Clutch Relay
Table 2: | Blower Motor Relay
Table 3: | Blower Motor Resistor Assembly
Table 4: | Heater And A/C Control Assembly
Table 5: | Heater And A/C Control Assembly

#### A/C Compressor Clutch Relay

Connector Part Information |

• | 12129716

• | 4-Way F Metri-Pack Series 280 FLX LK (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | PNK | 439 | Fuse Output-Ignition-1
85 | DK GRN/ WHT | 459 | Air Conditioning Control Relay Output-Coil
86 | PNK | 439 | Vehicle Speed Signal
87 | DK GRN | 59 | Air Conditioning Compressor Clutch Feed

#### Blower Motor Relay

Connector Part Information |

• | 12110539

• | 5-Way F Metri-Pack Series 280 FLX LK (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | PPL | 65 | Blower Motor Feed
85 | BRN | 64 | High Speed Blower Relay Feed-Coil
86 | BLK | 150 | Ground
87 | ORN | 840 | Fuse Output-Battery
87A | DK BLU | 101 | Blower Resistor-Output

#### Blower Motor Resistor Assembly

Connector Part Information |

• | 12129692

• | 4-Way F Metri-Pack Series 480 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 101 | Blower Resistor-Output
B | LT BLU | 72 | Blower Switch Output-Medium 2
C | TAN | 63 | Blower Switch Output-Medium
D | YEL | 60 | Blower Switch Output-Low

#### Heater And A/C Control Assembly

Connector Part Information |

• | 12020813

• | 5-Way F Metri-Pack Series 630 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 60 | Blower Switch Output-Low
B | BRN | 64 | High Speed Blower Relay Feed Coil
C | TAN | 63 | Blower Switch Output-Medium 1
D | LT BLU | 72 | Blower Switch Output-Medium 2
E | WHT | 119 | Mode Switch Output

#### Heater And A/C Control Assembly

Connector Part Information |

• | 12020557

• | 3-Way F Metri-Pack Series 480 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 66 | Outside Ambient Temperature Sensor Return
B | WHT | 119 | Mode Switch Output
C | BRN | 41 | Fuse Output-Ignition 3