For 1990-2009 cars

# RELEASE SOLENOID BOLTS MAY CONTACT TRUNK SILL PLATE-PROC.

#### SUBJECT: RELEASE SOLENOID ATTACHMENT BOLTS MAY CONTACT REAR TRUNK SILL PLATE - REPLACE HEAD SCREW

#### MODELS/YEARS: 1992 ACHIEVA

CONDITION: Release solenoid attachment bolts may contact rear trunk sill plate.

#### CORRECTION:

1. Remove existing hex head screw P/N 11504317.

2. Replace with torx head screw P/N11515144.

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation Number: R4020 Labor Time: See the Current Labor Time Guide Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.