For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Noise with ignition in NEUTRAL and the engine ON
1 |

1. Disassemble the transaxle case. Refer to Transmission Case Disassemble

• | The input gear bearing

• | The clutch release bearing

• | The speed gear bearing

• | The bearing races

• | The thrust surfaces

Are any of the componets worn or damaged?

Go to Step 2

Refer to Isolating Noise

2 | Service, repair, or replace any worn or damaged components. Refer to Transmission Case Disassemble Did the noise disappear? | System OK | Refer toIsolating Noise