For 1990-2009 cars

Servicing the front brakes usually corrects pulsation in the brake pedal. Service the rear brakes only if the problem persists.

In order to determine if the front or rear brakes are at fault, test drive the vehicle. Drive the vehicle at low speed in an area away from people and moving traffic, such as a large parking lot. Apply the park brake and feel for the pulsation. If a pulsation is not noticed, the fault is probably in the front brakes. When the brake drums are removed, thoroughly clean and inspect the drums for the following conditions:

• | Cracks

• | Scores

• | Deep grooves

• | Out-of-round

• | Taper

Normal, light scoring of brake drum surfaces not exceeding 1.5 mm (0.059 in.) in depth will not affect brake operation.