For 1990-2009 cars

#### Tires

Tires with unequal contact and unequal grip on road surfaces cause unequal braking. Ensure that the tires meet the following requirements:

• | Equally inflation

• | Identical in size

• | The tread pattern of the right and left tires must be approximately equal.

#### Vehicle Loading

A heavily loaded vehicle requires more braking effort. On a vehicle with unequal loading, the most heavily loaded wheels require more braking effort than the other wheels.

#### Wheel Alignment

Misalignment of the wheels, particularly excessive camber and caster, causes the brakes to pull to one side.

#### Trailer Towing

Towing a trailer requires longer braking distances and tends to overheat the brakes sooner.