For 1990-2009 cars

# REAR COMPARTMENT LID HINGE COVERS ARE LOOSE / RATTLE

#### SUBJECT: REAR COMPARTMENT LID HINGE COVERS ARE LOOSE/RATTLE (REPLACE PLASTIC LID HINGE COVER RETAINER/ADD FOAM PAD)

#### MODELS: 1994-95 BUICK SKYLARK 1994-95 OLDSMOBILE ACHIEVA 1994-95 PONTIAC GRAND AM

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE REAR COMPARTMENT LID HINGE COVERS ARE LOOSE/RATTLE OR HAVE FALLEN OFF.

#### CAUSE:

PLASTIC RETAINER IS WORN OUT.

#### CORRECTION:

TO CORRECT THIS CONDITION, REPLACE THE PLASTIC RETAINER WITH A METAL RETAINER AND ADD FOAM PAD TO REAR COMPARTMENT LID HINGE COVER USING THE FOLLOWING PROCEDURE.

1. REMOVE RH/LH REAR COMPARTMENT LID HINGE COVER. REFER TO FIGURE 1, ITEM 1.

2. REMOVE REAR COMPARTMENT LID HINGE COVER RETAINER. REFER TO FIGURE 1, ITEM 2.

3. INSTALL NEW REAR COMPARTMENT LID HINGE COVER RETAINER, P/N 22591829. REFER TO FIGURE 1, ITEM 2.

4. INSTALL A STICKY BACK FOAM PAD, 3 X 18 X 30MM, TO UNDERSIDE OF RH/LH REAR COMPARTMENT LID HINGE COVER BETWEEN THE RETAINER HOLE AND THE CROSS. REFER TO FIGURE 1, ITEM 3.

5. INSTALL RH/LH REAR COMPARTMENT LID HINGE COVER. REFER TO FIGURE 1, ITEM 1.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: C4605 (RIGHT) C4606 (LEFT) USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.