For 1990-2009 cars

# SMU - SECTION 8A, 8C1, 9D - REVISED LABEL DESCRIPTION

#### SUBJECT: SERVICE MANUAL UPDATE - SECTIONS 8A, 8C1, 9D - REVISED LABEL/DESCRIPTION OF CRANKLOW CIRCUIT (CKT 1350)

#### MODELS: 1996 BUICK SKYLARK 1996 OLDSMOBILE ACHIEVA 1996 PONTIAC GRAND AM

THIS BULLETIN IS TO REVISE PAGES 8A-80-6, 8A-133-0, 8C1-16 AND 9D-6 OF THE SERVICE MANUAL.

THE LABEL/DESCRIPTION OF THE CRANKLOW CIRCUIT (CKT 1350) IS NOT PROPERLY SHOWN IN THE SERVICE MANUAL. THE CRANKLOW CIRCUIT (CKT 1350) IS BETWEEN THE INSTRUMENT PANEL CLUSTER CONN C1, TERM "C7 (BUICK AND OLDSMOBILE)/TERM "C1" (PONTIAC) AND THE IGNITION SWITCH CONN C1, TERM "D". PLEASE LABEL THIS CIRCUIT AS FOLLOWS: .35 BLK, 1350. PLEASE UPDATE THE ABOVE LISTED PAGES ACCORDINGLY.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.