For 1990-2009 cars

### Removal Procedure

1. Remove the trim plate from the instrument panel cluster. Refer to Instrument Panel Lower Center Trim Replacement in Instrument Panel, Gauges, and Console.
2. Remove the fog lamp switch.

### Installation Procedure

1. Install the fog lamp switch.
2. Install the trim panel to the instrument panel cluster. Refer to Instrument Panel Lower Center Trim Replacement in Instrument Panel, Gauges, and Console.