For 1990-2009 cars

# Info - Air Conditioning Compressor Shaft Seal Replacement

Subject: | Air Conditioning Compressor Shaft Seal Replacement

Models: | 2001 Passenger Cars and Light Duty Trucks -- Except:

| Cadillac DeVille, Seville

| Chevrolet Metro, Prizm, Tracker, Venture

| Oldsmobile Aurora, Silhouette

| Pontiac Aztek, Montana

The procedure for replacing the compressor shaft seal has been deleted from the Electronic Service Information. The procedure outlined in any printed Service Manual for this operation and the associated special tools mentioned should be deleted from all printed Service Manuals in your possession.

Service of the compressor shaft seal on Delphi compressors is no longer an authorized service procedure. Special tools have not and will not be developed for this procedure. This applies to all 2001 Delphi compressors; V-5, V-7, HD6, HT6 and HU6.