For 1990-2009 cars

DTC | Description
--- | ---
DTC C1214 | DTC C1214 Brake Control Relay Contact Circuit Open
DTC C1215 | DTC C1215 Brake Control Relay Contact Circuit Active
DTC C1216 | DTC C1216 Brake Control Relay Coil Circuit Open
DTC C1217 | DTC C1217 Brake Control Relay Coil Circuit Short to Ground
DTC C1218 | DTC C1218 Brake Control Relay Coil Circuit Short to Voltage
DTC C1221 | DTC C1221 LF Wheel Speed Sensor Input Signal is 0
DTC C1222 | DTC C1222 RF Wheel Speed Sensor Input Signal is 0
DTC C1223 | DTC C1223 LR Wheel Speed Sensor Input Signal is 0
DTC C1224 | DTC C1224 RR Wheel Speed Sensor Input Signal is 0
DTC C1225 | DTC C1225 LF Excessive Wheel Speed Variation
DTC C1226 | DTC C1226 RF Excessive Wheel Speed Variation
DTC C1227 | DTC C1227 LR Excessive Wheel Speed Variation
DTC C1228 | DTC C1228 RR Excessive Wheel Speed Variation
DTC C1232 | DTC C1232 LF Wheel Speed Circuit Open or Shorted
DTC C1233 | DTC C1233 RF Wheel Speed Circuit Open or Shorted
DTC C1234 | DTC C1234 LR Wheel Speed Circuit Open or Shorted
DTC C1235 | DTC C1235 RR Wheel Speed Circuit Open or Shorted
DTC C1236 | DTC C1236 Low System Supply Voltage
DTC C1237 | DTC C1237 High System Supply Voltage
DTC C1238 | DTC C1238 Left Front ESB Does Not Hold Motor
DTC C1241 | DTC C1241 Right Front ESB Does Not Hold Motor
DTC C1242 | DTC C1242 Rear ESB Does Not Hold Motor
DTC C1243 | DTC C1243 Variable Effort Steering Steering Wheel Sensor Circuit Malfunction
DTC C1244 | DTC C1244 Left Front ABS Channel Does Not Move
DTC C1245 | DTC C1245 Right Front ABS Channel Does Not Move
DTC C1246 | DTC C1246 Rear ABS Channel Does Not Move
DTC C1247 | DTC C1247 Left Front ABS Motor Free Spins
DTC C1248 | DTC C1248 Right Front ABS Motor Free Spins
DTC C1251 | DTC C1251 Rear ABS Motor Free Spins
DTC C1252 | DTC C1252 LF ABS Channel in Release Too Long
DTC C1253 | DTC C1253 RF ABS Channel in Release Too Long
DTC C1254 | DTC C1254 Rear ABS Channel in Release Too Long
DTC C1255 | DTC C1255 EBCM Internal Malfunction
DTC C1256 | DTC C1256 Left Front ABS Motor Circuit Open
DTC C1257 | DTC C1257 LF ABS Motor Circuit Shorted to Ground
DTC C1258 | DTC C1258 LF ABS Motor Circuit Shorted to Voltage
DTC C1261 | DTC C1261 Right Front ABS Motor Circuit Open
DTC C1262 | DTC C1262 RF ABS Motor Circuit Shorted to Ground
DTC C1263 | DTC C1263 RF ABS Motor Circuit Shorted to Voltage
DTC C1264 | DTC C1264 Rear ABS Motor Circuit Open
DTC C1265 | DTC C1265 Rear ABS Motor Circuit Shorted to Ground
DTC C1266 | DTC C1266 Rear ABS Motor Circuit Shorted to Voltage
DTC C1267 | DTC C1267 DTC U1300 Previously Set
DTC C1268 | DTC C1268 DTC U1301 Previously Set
DTC C1273 | DTC C1273 VES Circuit Open or Shorted to Ground
DTC C1274 | DTC C1274 VES Circuit Shorted to Voltage
DTC C1275 | DTC C1275 PCM Requested ETS to Be Disabled
DTC C1276 | DTC C1276 LF Solenoid Circuit Open or Short to Ground
DTC C1277 | DTC C1277 LF Solenoid Circuit Shorted to Voltage
DTC C1278 | DTC C1278 RF Solenoid Circuit Open or Shorted to Ground
DTC C1281 | DTC C1281 RF Solenoid Circuit Shorted to Voltage
DTC C1282 | DTC C1282 Calibration Malfunction
DTC C1286 | DTC C1286 EBCM Turned On Brake Warning Indicator
DTC C1291 | DTC C1291 Open Brake Lamp Switch Contacts During Deceleration
DTC C1292 | DTC C1292 Open Brake Lamp Switch When ABS Was Required
DTC C1293 | DTC C1293 DTC C1291/C1292 Set in Current or Previous Ignition Cycle
DTC C1294 | DTC C1294 Brake Lamp Switch Circuit Always Active
DTC C1295 | DTC C1295 Brake Lamp Switch Circuit Open
DTC U1016 | DTC U1016 Loss of Communications with PCM in Data Link Communications
DTC U1255 | DTC U1255 Class 2 Communication Malfunction in Data Link Communications
DTC U1300 | DTC U1300 Class 2 Data Link Low in Data Link Communications
DTC U1301 | DTC U1301 Class 2 Data Link High in Data Link Communications