For 1990-2009 cars

Table 1: | Crankshaft Position (CKP) Sensor
Table 2: | Engine Coolant Temperature (ECT) Sensor
Table 3: | Evaporative Emission (EVAP) Canister Purge Solenoid
Table 4: | Evaporative Emission (EVAP) Canister Vent Solenoid
Table 5: | Fuel Injector 1
Table 6: | Fuel Injector 2
Table 7: | Fuel Injector 3
Table 8: | Fuel Injector 4
Table 9: | Fuel Pump and Sender Assembly
Table 10: | Fuel Tank Pressure (FTP) Sensor
Table 11: | Heated Oxygen Sensor (HO2S) Sensor 1
Table 12: | Heated Oxygen Sensor (HO2S) Sensor 2
Table 13: | Idle Air Control (IAC) Valve
Table 14: | Ignition Control Module (ICM)
Table 15: | Intake Air Temperature (IAT) Sensor
Table 16: | Knock Sensor (KS)
Table 17: | Manifold Absolute Pressure (MAP) Sensor
Table 18: | Throttle Position (TP) Sensor

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 12162192

• | 2-Way F Metri-Pack 150.2 Series Pull-to-Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 574 | Low Reference
B | YEL | 573 | CKP Sensor 1 Signal

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | 12162192

• | 2-Way F Metri-Pack 150.2 Series Pull-to-Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 2761 | Low Reference
B | YEL | 410 | ECT Sensor Signal

#### Evaporative Emission (EVAP) Canister Purge Solenoid

Connector Part Information |

• | 12052637

• | 2-Way F Metri-Pack 150 Series Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Ignition 3 Voltage
B | DK GRN/ WHT | 428 | EVAP Canister Purge Solenoid Control

#### Evaporative Emission (EVAP) Canister Vent Solenoid

Connector Part Information |

• | 12059862

• | 2-Way F Metri-Pack 150 Series Sealed (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Ignition 3 Voltage
B | WHT | 1310 | EVAP Canister Vent Solenoid Control

#### Fuel Injector 1

Connector Part Information |

• | 15326180

• | 2-Way F Micro-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 839 | Ignition 1 Voltage
B | BLK | 1744 | Fuel Injector 1 Control

#### Fuel Injector 2

Connector Part Information |

• | 15326180

• | 2-Way F Micro-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 839 | Ignition 1 Voltage
B | LT GRN/ BLK | 1745 | Fuel Injector 2 Control

#### Fuel Injector 3

Connector Part Information |

• | 15326180

• | 2-Way F Micro-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 839 | Ignition 1 Voltage
B | PNK/BLK | 1746 | Fuel Injector 3 Control

#### Fuel Injector 4

Connector Part Information |

• | 15326180

• | 2-Way F Micro-Pack 64 Series Sealed (BLK)

A | PNK | 839 | Ignition 1 Voltage
B | LT BLU/ BLK | 844 | Fuel Injector 4 Control

#### Fuel Pump and Sender Assembly

Connector Part Information |

• | 12059110

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 150 | Ground
B | GRY | 120 | Fuel Pump Supply Voltage

#### Fuel Tank Pressure (FTP) Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Low Reference
B | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
C | GRY | 2709 | 5 Volt Reference

#### Heated Oxygen Sensor (HO2S) Sensor 1

Connector Part Information |

• | 12160479

• | 4-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 1667 | HO2S Low Signal (Bank 1 Sensor 1)
B | PPL | 1666 | HO2S High Signal (Bank 1 Sensor 1)
C | DK GRN | 676 | HO2S Heater Low Control (Bank 1 Sensor 1)
D | PNK | 1039 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) Sensor 2

Connector Part Information |

• | 15326423

• | 4-Way M Metri-Pack 150 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1669 | HO2S Low Signal (Bank 1 Sensor 2)
B | PPL/WHT | 1668 | HO2S High Signal (Bank 1 Sensor 2)
C | BLK/WHT | 1423 | HO2S Heater Low Control (Bank 1 Sensor 2)
D | BRN | 241 | Ignition 3 Voltage

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 15354717

• | 4-Way F Global Terminal 150 Sealed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/ BLK | 444 | IAC Coil B Low Control
B | LT GRN/ WHT | 1749 | IAC Coil B High Control
C | LT BLU/ BLK | 1748 | IAC Coil A Low Control
D | LT BLU/ WHT | 1747 | IAC Coil A High Control

#### Ignition Control Module (ICM)

Connector Part Information |

• | 15326098

• | 9-Way F Global Terminal 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 239 | Ignition 1 Voltage
B | WHT | 423 | IC Timing Control
C-D | -- | -- | Not Used
E | BLK | 450 | Ground
F | BRN/WHT | 633 | CMP Sensor Signal
G | ORN | 406 | IC Timing Control B
H-J | -- | -- | Not Used

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 12162196

• | 2-Way F Metri-Pack 150.2 Series Pull-to-Seat Sealed (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2760 | Low Reference
B | TAN | 472 | IAT Sensor Signal

#### Knock Sensor (KS)

Connector Part Information |

• | 12077901

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 496 | Knock Sensor Signal
B | GRY | 1716 | Low Reference

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | 12129945

• | 3-Way F Metri-Pack 150 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Low Reference
B | LT GRN | 432 | MAP Sensor Signal
C | GRY | 2704 | 5 Volt Reference

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 15326807

• | 3-Way F Global Terminal 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY/BLK | 2701 | 5 Volt Reference
B | BLK | 2752 | Low Reference
C | DK BLU | 417 | TP Sensor Signal