For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
Schematic Reference: Instrument Cluster Schematics
1 | Did you perform the Instrument Cluster Diagnostic System Check? | -- | Go to Step 2 | Go to Diagnostic System Check - Instrument Cluster
2 |

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.
3. With a scan tool, observe the Engine Oil Life Remaining parameter in the PCM Engine Data 3 2.4L or Engine Data 2 3.4L list.

Does the Engine Oil Life parameter display less than the specified value?

11%

Go to Step 3

System OK

3 | Replace the IPC. Refer to Instrument Cluster Replacement . Did you complete the replacement? | -- | Go to Step 4 | --
4 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 2