For 1990-2009 cars

The steering wheel and column has 3 primary functions:

• | Vehicle steering

• | Driver convenience

• | Driver safety

### Vehicle Steering

The steering wheel is the first link between the driver and the vehicle. The steering wheel is fastened to a steering shaft within the column. At the lower end of the column, the intermediate shaft connects the column to the steering gear.

### Driver Convenience

The steering wheel and column may also have driver controls attached for convenience and comfort. The following controls may be mounted on or near the steering wheel or column.

• | The turn signal switch

• | The hazard switch

• | The headlamp dimmer switch

• | The wiper/washer switch

• | The horn pad/cruise control switch

• | The redundant radio/entertainment system controls

• | The tilt or tilt/telescoping functions

### Driver Safety

The energy-absorbing steering column compresses in the event of a front-end collision, which reduces the chance of injury to the driver. The mounting capsules break away from the mounting bracket in the event of an accident.