For 1990-2009 cars

# Info - Pressure Control Solenoid Replacement for 4T65-E, 4T40-E and 4T45-E Transmission/Transmission

Subject: | Pressure Control Solenoid Replacement for 4T65-E, 4T40-E, and 4T45-E Transaxle/Transmission

Models: | 2000-2003 Buick Century, LeSabre, Park Avenue, Regal

| 2002-2003 Buick Rendezvous

| 2000-2001 Chevrolet Lumina

| 2000-2003 Chevrolet Cavalier, Impala, Malibu, Monte Carlo, Venture

| 2000-2002 Oldsmobile Intrigue

| 2000-2003 Oldsmobile Alero, Silhouette

| 2000-2003 Pontiac Bonneville, Grand Am, Grand Prix, Montana, Sunfire

| 2001-2003 Pontiac Aztek

| with RPO Codes MN4, MN5, M13, M15, MN3, MN7or M76

The pressure control solenoid in the above transaxles has changed for the 2003 models.

Important: While the physical dimensions will allow usage of the new solenoid in past model transaxles or usage of the old solenoid in 2003 model transaxles, they should not be interchanged. Interchanging of the pressure control solenoids will result in improper shift characteristics, customer dissatisfaction, and needed repeat repairs.

When replacing a pressure control solenoid, be sure to use the correct part number.

Model Year | Manufacturer | P/N
--- | --- | ---
2000 - 2002 | Delphi | 10478146
2003 | Bosch | 24225825

Parts are currently available from GMSPO.