For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Lateral Link to Knuckle Nut | 100 N·m | 74 lb ft
Lateral Link to Rear Suspension Support Bolt | 100 N·m | 74 lb ft
Parking Brake Cable Bracket Bolts | 10 N·m | 89 lb in
Rear Suspension Strut Nut | 70 N·m | 52 lb ft
Rear Suspension Support Mounting Bolt | 120 N·m | 89 lb ft
Rear Wheel Hub to Knuckle Bolt | 85 N·m | 62 lb ft
Stabilizer Shaft Bracket to Rear Suspension Support Nut | 53 N·m | 39 lb ft
Stabilizer Shaft Link Bolt to Knuckle | 51 N·m | 37 lb ft
Strut-to-Knuckle Nut | 120 N·m | 89 lb ft
Strut Mount-to-Body Nut | 25 N·m | 18 lb ft
Trailing Arm to Body Bolt

- First Pass

65 N·m

48 lb ft

- Final Pass

+120°

Trailing Arm to Knuckle Bolt | 69 N·m | 51 lb ft