For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console trim plate. Refer to Front Floor Console Trim Plate Replacement in Instrument Panel, Gages, and Console.
2. Rotate the shift control indicator lamp socket (4) counterclockwise. Remove the socket from the trim plate (1).
3. Remove the bulb from the socket.

### Installation Procedure

1. Install the bulb to the socket.
2. Install the shift control indicator lamp socket (4) to the trim plate (1). Rotate the socket clockwise to secure.
3. Install the front floor console trim plate. Refer to Front Floor Console Trim Plate Replacement in Instrument Panel, Gages, and Console.