For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Pipe Fittings at Brake Pressure Modulator Valve (BPMV) and Master Cylinder | 23.0 N·m | 17 lb ft
Console Trim Plate Screws | 2 N·m | 18 lb in
Electronic Brake Control Module (EBCM) Assembly Retaining Nuts | 10.0 N·m | 89 lb in
Electronic Brake Control Module (EBCM) Mounting Screw | 11.0 N·m | 97 lb in
Hydraulic Modulator Bracket Mounting Bolt | 24.0 N·m | 18 lb ft
Hydraulic Modulator Mounting Nut | 30.0 N·m | 22 lb ft
Screws, EBCM to BPMV | 5 N·m | 44 lb in