For 1990-2009 cars

#### No Park

Checks | Causes
--- | ---
Parking Lock Actuator Assembly (807) |

• | Bent or damaged rod

• | Binding or broken spring

• | The rod is not attached to the detent lever

Detent Roller and Spring (804) |

• | The bolt is not torqued, or loose

• | Bent or damaged

Detent Lever (806) |

• | Damaged or loose

• | A manual shaft pin is missing

Manual Valve (800) |

• | Misaligned

• | The manual valve to detent lever link is bent

Parking Lock Pawl (663) |

• | Damaged

• | Broken tooth

Park Lock Gear (659) |

• | Damaged teeth

• | Damaged splines

Park Pawl Spring (662) | Broken or missing
Shift Linkage | Misadjusted