For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specification
--- | ---
Metric | English
Drain Plugs | 38 N·m | 28 lb ft
Intermediate Shaft Bolt | 95 N·m | 70 lb ft
Output Shaft Bearing Race Bolt | 12 N·m | 106 lb in
Rear Cover Bolts | 25 N·m | 18 lb ft
Reverse Lockout Bolt | 6 N·m | 53 lb in
Reverse Switch | 18 N·m | 13 lb ft
Ring Gear | 90 N·m | 66 lb ft
Shaft Bolts | 110 N·m | 81 lb ft
Shifter Guide Bolt | 25 N·m | 18 lb ft
Shifter Retaining Bolts | 25 N·m | 18 lb ft
Speed Sensor | 12 N·m | 106 lb in
Transmission Housing Bolts | 27 N·m | 20 lb ft
Vent Cap | 5 N·m | 44 lb in