For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the run channel weather strip from the window (1). Refer to Window Channel Replacement .
3. Remove the front window. Refer to Front Side Door Window Replacement .
4. Remove the rear run channel bolt (2). Remove the channel (1).

### Installation Procedure

1. Install the rear run channel (1). Secure with the channel bolt (2).
2. Install the front window . Refer to Front Side Door Window Replacement .
3. Install the run channel weather strip to the window (1). Refer to Window Channel Replacement .
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .