For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accel. Cable Bracket Bolts | 12 N·m | 106 lb in
Accel. Cable Bracket Nut | 26 N·m | 19 lb in
Air Cleaner Outlet Resonator Clamp | 5 N·m | 44 lb in
Air Cleaner Outlet Resonator Mounting Screws | 6 N·m | 53 lb in
Accel. Pedal Nuts | 30 N·m | 25 lb in
CKP Sensor Bolts | 10 N·m | 88 lb in
CMP Sensor Bolts | 15 N·m | 11 lb ft
Engine Oil Pressure Sensor | 12 N·m | 106 lb in
EVAP Canister Retainer Attaching Bolt | 10 N·m | 88 lb in
Flex Duct Clamps | 5 N·m | 44 lb in
Fuel Filter Fitting | 27 N·m | 20 lb ft
Fuel Pipe Clamp Bolt | 12 N·m | 106 lb in
Fuel Pipe Fittings | 27 N·m | 20 lb in
Fuel Inlet Pipe Nut | 30 N·m | 22 lb in
Fuel Line Clamp Screws | 10 N·m | 89 lb in
Fuel line Fitting to Fuel Rail | 27 N·m | 20 lb in
Fuel Pressure Regulator Retainer Screw | 6 N·m | 53 lb in
Fuel Rail Attaching Bolts | 24 N·m | 18 lb in
HO2S 2 | 41 N·m | 30 lb in
ICM Cover Bolts | 22 N·m | 16 lb in
ICM Screws | 4 N·m | 35 lb in
Idle Air Control Valve | 3 N·m | 27 lb in
Ignition Coil Housing Screws | 4 N·m | 35 lb in
Idle Air Control Valve | 3 N·m | 27 lb in
Knock Sensor | 25 N·m | 18 lb ft
Lower Air Cleaner Mounting Bolt | 6 N·m | 53 lb in
MAP Sensor Attaching Screw | 6.5 N·m | 53 lb in
Muffler Hanger Bolt | 15 N·m | 11 lb in
O2S 1 | 41 N·m | 30 lb in
Outlet Pipe Bracket | 6 N·m | 53 lb in
PCM Retainer Attaching Bolts | 10 N·m | 88 lb in
PCM Electrical Connector Screws | 8 N·m | 71 lb in
Purge Valve Mounting Bracket Attaching Bolt | 8 N·m | 71 lb in
Regulator Retainer | 11.5 N·m | 102 lb in
Resonator Attaching Bolt | 6 N·m | 53 lb in
Separator and Solenoid Attaching Bolts | 8 N·m | 71 lb in
Spark Plugs | 18 N·m | 13 lb in
Tank Retaining Straps Bolt | 35 N·m | 26 lb in
Throttle Body Attaching Bolts | 6.5 N·m | 58 lb in
Throttle Position Sensor | 2 N·m | 18 lb in
TP Sensor Mounting Screws | 3 N·m | 27 lb in
Upper Air Cleaner Cover Screws | 3 N·m | 27 lb in