For 1990-2009 cars

### Removal Procedure

1. Remove the washer solvent container. Refer to Windshield Washer Solvent Container Replacement .
2. Disconnect the electrical connector from the washer pump.
3. Disconnect the hose from the washer pump.
4. Remove the washer pump from the washer solvent container.

### Installation Procedure

1. Install the washer pump in the washer solvent container assembly.
2. Connect the hose to the washer pump.
3. Connect the electrical connector to the washer pump.
4. Install the washer solvent container. Refer to Windshield Washer Solvent Container Replacement .