For 1990-2009 cars

Figure 1: |

#### Front of Engine - 1 of 2

(1) | Manifold Absolute Pressure (MAP) Sensor
(2) | Engine Coolant Temperature (ECT) Sensor
(3) | Idle Air Control (IAC) Valve
(4) | Throttle Position (TP) Sensor

Figure 2: |

#### Front of Engine - 2 of 2

(1) | Intake Air Temperature (IAT) Sensor
(2) | Ignition Control Module (ICM)
(3) | Interconnect
(4) | Knock Sensor (KS)
(5) | C102

Figure 3: |

#### Upper Right Side of the Engine

(1) | Brake Fluid Reservoir
(2) | Evaporative Emission (EVAP) Canister Purge Solenoid

Figure 4: |

#### Fuel Injection System

(1) | C130
(2) | Fuel Injector 1
(3) | Fuel Injector 2
(4) | Fuel Injector 3
(5) | Fuel Injector 4

Figure 5: |

#### Ignition System

(1) | Ignition Control Module (ICM)
(2) | Interconnect

Figure 6: |

#### Crankshaft Position (CKP) Sensor

(1) | Crankshaft Position (CKP) Sensor

Figure 7: |

#### Heated Oxygen Sensor (HO2S) Sensor 1

(1) | Heated Oxygen Sensor (HO2S) Sensor 1

Figure 8: |

#### Left Side of Passenger Compartment

(1) | Fuse Block - Left I/P
(2) | C500
(3) | C501
(4) | Seat Belt Switch Connector
(5) | C306
(6) | G301
(7) | C300
(8) | Powertrain Control Module (PCM)

Figure 9: |

#### Evaporative Emission (EVAP) Canister Vent Solenoid

(1) | Evaporative Emission (EVAP) Canister Vent Solenoid

Figure 10: |

#### Heated Oxygen Sensor (HO2S) Sensor 2

(1) | Heated Oxygen Sensor (HO2S) Sensor 2

Figure 11: |

#### Fuel Pump and Sender Assembly

(1) | Fuel Tank Pressure (FTP) Sensor
(2) | Fuel Pump and Sender Assembly
(3) | Fuel Level Sensor