For 1990-2009 cars

### Diagnostic Aids

When hydraulic fluid is present on the master cylinder and dust cover and the clutch pedal assembly, check for worn or damage seals or other faulty parts of the clutch master cylinder.

### Test Description

The number(s) below refer to the step number(s) on the diagnostic table.

1. This step explains there parts and the operation of the clutch system.

2. This step checks for any seal leaks from the master cylinder.

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: Hydraulic fluid is present in the master cylinder dust cover and on the clutch pedal assembly.
1 | Did you review the clutch symptom operations and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Clutch
2 | Inspect the master cylinder seal for any hydraulic fluid leaks. Does the clutch master cylinder seal have any leaks? | Go to Step 3 | System OK
3 | Replace the clutch master cylinder. Refer to Clutch Actuator Cylinder Replacement . Did you find and repair the condition? | Go to Step 4 | Go to Diagnostic Aids
4 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 1