For 1990-2009 cars

#### A/T Shift Lock Control Solenoid

Connector Part Information |

• | 12052832

• | 2-Way F Metri Pack 150 Series (BLK)

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
A | DK GRN/WHT | 1135 | A/T Shift Lock Solenoid Supply Voltage
B | BLK | 250 | Ground

#### Park/Neutral Position (PNP) Switch, C1

Connector Part Information |

• | 12191757

• | 4-Way F Metri Pack 150 Series Sealed (WHT)

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
A | WHT | 776 | Transmission Range Switch Signal P
B | YEL | 772 | Transmission Range Switch Signal B
C | GRY | 773 | Transmission Range Switch Signal C
D | BLK/WHT | 771 | Transmission Range Switch Signal A

#### Park/Neutral Position (PNP) Switch, C2

Connector Part Information |

• | 12129840

• | 7-Way F Metri Pack 150/280 Series Sealed (GRY)

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | PNK | 539 | Ignition 1 Voltage
C | LT GRN | 275 | Neutral Safety Switch Park Signal
D | BLK/WHT | 451 | Ground
E | PPL | 6 | Starter Solenoid Crank Voltage
F | LT GRN | 24 | Backup Lamp Supply Voltage
G | YEL | 5 | Crank Voltage

#### Stoplamp Switch, C1

Connector Part Information |

• | 12033701

• | 2-Way F Metri Pack 480 Series (GRY)

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
A | ORN | 140 | Battery Positive Voltage
B | LT BLU | 20 | Stoplamp Supply Voltage

#### Stoplamp Switch, C2

Connector Part Information |

• | 12033706

• | 4-Way F Metri Pack 280 Series (BLU)

Pin | Wire Color | CKT No. | Function
--- | --- | --- | ---
A | LT GRN | 275 | Neutral Safety Switch Park Signal
B | DK GRN/WHT | 1135 | A/T Shift Lock Solenooid Supply Voltage
C-D | -- | -- | Not Used