For 1990-2009 cars

## Parking and Turn Signal Lamp Replacement Pontiac

### Removal Procedure

1. Remove the tail lamp. Refer to Tail Lamp Replacement .
2. Disconnect the electrical connector.
3. Remove the bulb from the socket.

Twist the bulb and pull outward.

### Installation Procedure

1. Install the bulb.

Push the bulb inward and twist until the bulb is retained.

2. Connect the electrical connector.
3. Install the tail lamp. Refer to Tail Lamp Replacement .

## Parking and Turn Signal Lamp Replacement Oldsmobile

### Removal Procedure

1. Remove the tail lamps. Refer to Tail Lamp Replacement .
2. Disconnect the electrical connector.
3. Remove the bulb from the socket.

Twist the bulb and pull outward.

### Installation Procedure

1. Install the bulb.

Push the bulb inward and twist until the bulb is retained.

2. Connect the electrical connector.
3. Install the tail lamp. Refer to Tail Lamp Replacement .