For 1990-2009 cars

DTC | Descriptor
--- | ---
DTC B0016 | RF/Passenger Frontal Deployment Loop (Single Stage or Stage 1) Resistance Low
DTC B0017 | RF/Passenger Frontal Deployment Loop (Single Stage or Stage 1) Open
DTC B0018 | RF/Passenger Frontal Deployment Loop (Single Stage or Stage 1) Short to Ground/Voltage Out of Range
DTC B0022 | LF/Driver Frontal Deployment Loop (Single Stage or Stage 1) Resistance Low
DTC B0024 | LF/Driver Frontal Deployment Loop (Single Stage or Stage 1) Short to Ground/Voltage Out of Range
DTC B0026 | LF/Driver Frontal Deployment Loop (Single Stage or Stage 1) Open
DTC B0051 | Deployment Commanded
DTC B0053 | Deployment Commanded with Loop Malfunctions Present
DTC B1000 | BCM Malfunction
DTC B1001 | Option Configuration Error
DTC B1365 | Device Ignition 0 Circuit
DTC B1369 | Ignition 0 Fault
DTC B1374 | Ignition 1 Fault
DTC B1379 | Ignition 3 Fault
DTC B1780 | Theft Lock
DTC B2532 | Front Foglamp Relay Out Short to Ground/Open
DTC B2533 | Front Foglamp Relay Output Short to Bat
DTC B2558 | Interior Lamp Control Output Short to Battery
DTC B2575 | Headlamp Request/Feedback Mismatch
DTC B2577 | Headlamp Control Circuit Low
DTC B2578 | Headlamp Relay Output Short to Battery
DTC B2585 | Parklamp Control Circuit Malfunction
DTC B2587 | Parklamp Relay Output Short to Ground/Op
DTC B2588 | Parklamp Relay Output Short to Battery
DTC B2600 | DRL Error
DTC B2601 | DRL Stuck
DTC B2602 | DRL Relay Output Short to Ground/Open
DTC B2603 | DRL Relay Output Short to Battery
DTC B2647 | Ambient Light Sensor Circuit Low
DTC B2648 | Ambient Light Sensor Circuit High
DTC B2752 | Horn Relay Coil Circuit Low
DTC B2753 | Horn Relay Coil Circuit High
DTC B2947 | Security System Sensor Power CKT Low
DTC B2948 | Security System Sensor Power CKT High
DTC B2957 | Security System Sensor Data Circuit Low
DTC B2958 | Security System Sensor Data Circuit High
DTC B2960 | Sec Sys Sensor Data Incorrect but Valid
DTC B2965 | Key In Ignition Fault
DTC B3031 | Security System Controller in Learn Mode
DTC B3033 | Security System Indicates Tamper
DTC B3127 or B3128 | Driver Door Unlock Circuit
DTC B3132 or B3133 | Door Unlock Circuit
DTC B3137 or B3138 | All Door Lock Circuit
DTC B3267 | Decklid Relay Output Short to Ground/Open
DTC B3268 | Decklid Relay Output Short to Battery
DTC C1214 | Solenoid Valve Relay Coil Contact Circuit Open
DTC C1217 | Pump Motor Shorted to Ground
DTC C1218 | Pump Motor Circuit Shorted to Voltage or Motor Ground Open
DTC C1221-C1235 | Wheel Speed Sensor Circuit
DTC C1236 | Low System Supply Voltage
DTC C1237 | High System Supply Voltage
DTC C1241 | Variable Effort Steering Malfunction
DTC C1242 or C1243 | Pump Motor Circuit
DTC C1245 | Low Tire Pressure Detected
DTC C1247 | Low Brake Fluid Detected
DTC C1254 | Abnormal Shutdown Detected
DTC C1255 or C1256 | ECU Malfunction
DTC C1261-C1268 | EBCM Internal Solenoid Circuit
DTC C1275 | PCM Requested ETS to Be Disabled
DTC C1278 | RF Solenoid Circuit Open or Shorted to Ground
DTC C1287 | Steering Position Sensor Circuit
DTC C1295 | Brake Lamp Switch Circuit Open
DTC C1298 | PCM Indicated Class 2 Serial Data Link Malfunction
DTC P0030 | HO2S Heater Control Circuit Sensor 1
DTC P0101 | Mass Air Flow (MAF) Sensor Performance
DTC P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency
DTC P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency
DTC P0105 | Manifold Absolute Pressure (MAP) Sensor Performance/Range
DTC P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage
DTC P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage
DTC P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage
DTC P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage
DTC P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage
DTC P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage
DTC P0121 | Throttle Position (TP) Sensor Performance
DTC P0122 | Throttle Position (TP) Sensor Circuit Low Voltage
DTC P0123 | Throttle Position (TP) Sensor Circuit High Voltage
DTC P0125 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop Fuel Control
DTC P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature
DTC P0130 | O2S Circuit Closed Loop (CL) Performance Sensor 1
DTC P0131 | HO2S Circuit Low Voltage Sensor 1
DTC P0132 | HO2S Circuit High Voltage Sensor 1
DTC P0133 | HO2S Slow Response Sensor 1
DTC P0134 | HO2S Circuit Insufficient Activity Sensor 1
DTC P0135 | HO2S Heater Performance Sensor 1
DTC P0137 | HO2S Circuit Low Voltage Sensor 2
DTC P0138 | HO2S Circuit High Voltage Sensor 2
DTC P0140 | HO2S Circuit Insufficient Activity Sensor 2
DTC P0141 | HO2S Heater Performance Sensor 2
DTC P0171 | Fuel Trim System Lean
DTC P0172 | Fuel Trim System Rich
DTC P0201-P0204 | Injector Control Circuit
DTC P0201-P0206 | Injector Control Circuit
DTC P0218 | Transmission Fluid Overtemperature
DTC P0230 | Fuel Pump Relay Control Circuit
DTC P0300 | Engine Misfire Detected
DTC P0301-P0304 | Engine Misfire Detected
DTC P0325 | Knock Sensor (KS) Circuit
DTC P0327 | Knock Sensor (KS) Circuit
DTC P0336 | Crankshaft Position (CKP) Sensor Performance
DTC P0340 | CMP Sensor Circuit Low Input
DTC P0341 | Camshaft Position (CMP) Sensor Performance
DTC P0401 | Exhaust Gas Recirculation (EGR) Flow Insufficient
DTC P0403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit
DTC P0404 | Exhaust Gas Recirculation (EGR) Open Position Performance
DTC P0405 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage
DTC P0420 | Catalyst System Low Efficiency
DTC P0440 | Evaporative Emission (EVAP) System
DTC P0442 | Evaporative Emission (EVAP) System Small Leak Detected
DTC P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit
DTC P0446 | Evaporative Emission (EVAP) Vent System Performance
DTC P0449 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit
DTC P0452 | Fuel Tank Pressure Sensor Circuit Low Voltage
DTC P0453 | Fuel Tank Pressure Sensor Circuit High Voltage
DTC P0461 | Fuel Level Sensor Performance
DTC P0462 | Fuel Level Sensor Circuit Low Voltage
DTC P0463 | Fuel Level Sensor Circuit High Voltage
DTC P0480 | Cooling Fan Relay 1 Control Circuit
DTC P0481 | Cooling Fan Relay 2 Control Circuit
DTC P0502 | Vehicle Speed Sensor (VSS) Circuit Low Input
DTC P0503 | Vehicle Speed Sensor (VSS) Circuit Intermittent
DTC P0506 | Idle Speed Low
DTC P0507 | Idle Speed High
DTC P0530 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit
DTC P0562 | System Voltage Low
DTC P0563 | System Voltage High
DTC P0601 | Control Module Read Only Memory (ROM)
DTC P0601-P0607, P1600, P1621, P1627, P1680, P1681, or P1683 | ECU Malfunction
DTC P0602 | Control Module Not Programmed
DTC P0620 | Generator Performance
DTC P0621 | Generator L-Terminal Circuit
DTC P0622 | Generator F-Terminal Circuit
DTC P0650 | Malfunction Indicator Lamp (MIL) Control Circuit
DTC P0705 | Transmission Range Switch Circuit
DTC P0711 | TFT Sensor Circuit Range/Performance
DTC P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Input
DTC P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Input
DTC P0716 | Input Speed Sensor Circuit Intermittent
DTC P0717 | Input Speed Sensor Circuit Low Input
DTC P0719 | Brake Switch Circuit Low Input
DTC P0724 | Brake Switch Circuit High Input
DTC P0730 | Incorrect Gear Ratio
DTC P0741 | TCC System Stuck Off
DTC P0742 | TCC System Stuck On
DTC P0748 | Pressure Control Solenoid Circuit Electrical
DTC P0751 | 1-2 Shift Solenoid Valve Performance
DTC P0752 | 1-2 Shift Solenoid Valve Performance - No Second or Third Gear
DTC P0753 | 1-2 Shift Solenoid Circuit Electrical
DTC P0756 | 2-3 Shift Solenoid Valve Performance
DTC P0757 | 2-3 Shift Solenoid Valve Performance - No Third or Fourth Gear
DTC P0758 | 2-3 Shift Solenoid Circuit Electrical
DTC P1106 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent High Voltage
DTC P1107 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent Low Voltage
DTC P1111 | Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage
DTC P1112 | Intake Air Temperature (IAT) Sensor Circuit Intermittent Low Voltage
DTC P1114 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent Low Voltage
DTC P1115 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent High Voltage
DTC P1121 | Throttle Position (TP) Sensor Circuit Intermittent High Voltage
DTC P1122 | Throttle Position (TP) Sensor Circuit Intermittent Low Voltage
DTC P1133 | HO2S Insufficient Switching Sensor 1
DTC P1134 | HO2S Transition Time Ratio Sensor 1
DTC P1137 | HO2S Circuit Low Voltage During Power Enrichment Sensor 2
DTC P1138 | HO2S Circuit High Voltage During Decel Fuel Cutoff Sensor 2
DTC P1171 | Fuel System Lean During Acceleration
DTC P1189 | Engine Oil Pressure (EOP) Switch Circuit
DTC P1336 | Crankshaft Position (CKP) System Variation Not Learned
DTC P1351 | Ignition Coil Control Circuit High Voltage
DTC P1352 | Ignition Bypass Circuit High Voltage
DTC P1361 | Ignition Control (IC) Circuit Low Voltage
DTC P1362 | Ignition Bypass Circuit Low Voltage
DTC P1374 | Crankshaft Position (CKP) High to Low Resolution Frequency Correlation
DTC P1380 | Misfire Detected - Rough Road Data Not Available
DTC P1381 | Misfire Detected - No Communication with Brake Control Module
DTC P1404 | Exhaust Gas Recirculation (EGR) Closed Position Performance
DTC P1441 | Evaporative Emission (EVAP) System Flow During Non-Purge
DTC P1546 | Air Conditioning (A/C) Clutch Relay Control Circuit
DTC P1554 | Cruise Control Feedback Circuit
DTC P1585 | Cruise Control Inhibit Output Circuit
DTC P1626 | Theft Deterrent Fuel Enable Signal Lost
DTC P1630 | Theft Deterrent Learn Mode Active
DTC P1631 | Theft Deterrent Start Enable Signal Not Correct
DTC P1632 | Theft Deterrent Fuel Disable Signal Received
DTC P1635 | 5 Volt Reference 1 Circuit
DTC P1639 | 5 Volt Reference 2 Circuit
DTC P1640 | Control Module Output A Circuit
DTC P1650 | Control Module Output B Circuit
DTC P1660 | Control Module Output C Circuit
DTC P1670 | Control Module Output D Circuit
DTC P1810 | TFP Valve Position Switch Circuit
DTC P1811 | Maximum Adapt and Long Shift
DTC P1860 | TCC PWM Solenoid Circuit Electrical
DTC P1887 | TCC Release Switch Circuit
DTC U1000 and U1255 | Class 2 Communication Malfunction
DTC U1001-U1254 | Loss of XXX Communications
DTC U1300 | Class 2 Data Link Low
DTC U1301 | Class 2 Data Link High