For 1990-2009 cars

#### Electronic Brake Control Module (EBCM)

Scan Tool Output Control | Additional Menu Selections | Description
--- | --- | ---
ABS Relay | -- | Commands the ABS relay ON and OFF
Automated Bleed | -- | Used in order to bleed the ABS hydraulics-Refer to Antilock Brake System Automated Bleed Procedure .
Automated Test | -- | Cycles each solenoid valve and the pump motor in order to verify component operation. This test is identical to the Initialization Sequence. If a malfunction is detected, the EBCM will set the appropriate DTCs. The DTCs will be displayed upon completion of the test.
LF Inlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF
LF Outlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF
LR Inlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF
LR Outlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF
RF Inlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF
RF Outlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF
RR Inlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF
RR Outlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF