For 1990-2009 cars

Important: Review the system operation in order to familiarize yourself with the system functions.

Refer to Wiper/Washer System Description and Operation .

### Visual/Physical Inspection

• | Inspect for aftermarket devices which could affect the operation of the Windshield Wiper/Washer System. Refer to Checking Aftermarket Accessories in Wiring Systems.

• | Inspect the easily accessible or visible system components for obvious damage or conditions which could cause the symptom.

• | Inspect the washer fluid reservoir for the proper fluid level.

### Intermittent

Faulty electrical connections or wiring may be the cause of intermittent conditions. Refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems.

### Symptom List

Refer to a symptom diagnostic procedure from the following list in order to diagnose the symptom:

• | Low Washer Fluid Indicator Malfunction

• | Washers Always On

• | Washers Inoperative

• | Wipers Always On

• | Wipers Inoperative - All Modes

• | Wipers Inoperative - One or More Modes