For 1990-2009 cars

Figure 1: |

#### Battery

(1) | Positive Battery Cable
(2) | Negative Battery Cable
(3) | Battery Ground
(4) | Engine Ground
(5) | Fuse Block -- Underhood

Figure 2: |

#### Starter

(1) | To A/C Compressor Clutch
(2) | Positive Battery Cable
(3) | Starter Solenoid
(4) | Starter Solenoid Ground
(5) | Starter
(6) | Battery Positive

Figure 3: |

#### Right Hand Front of Engine

(1) | Generator
(2) | Generator Lead
(3) | Ground Splice Pack
(4) | Ground Splice Pack
(5) | Engine Wiring Harness
(6) | Evaporative Emission (EVAP) Canister Purge Solenoid
(7) | A/C Compressor Clutch Connector
(8) | A/C Compressor Clutch
(9) | Generator Connector