For 1990-2009 cars

### Diagnostic Aids

When hydraulic fluid is present on the actuator or on the cylinder body, check for worn or damage seals or other faulty parts of the concentric slave cylinder.

### Test Description

The number(s) below refer to the step number(s) on the diagnostic table.

1. This step explains there parts and the operation of the clutch system.

2. This step checks for any seal leaks from the clutch actuator.

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: Hydraulic fluid is in the concentric slave cylinder area or on the cylinder body.
1 | Did you review the clutch symptom operations and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Clutch
2 | Remove the transmission. Refer to Transmission Replacement .Inspect the concentric slave cylinder for fluid leaks. Is there a leak on the actuator cylinder? | Go to Step 3 | System OK
3 | Replace the clutch actuator. Refer to Clutch Actuator Cylinder Replacement . Did you find and repair the condition? | Go to Step 4 | Go to Diagnostic Aids
4 | Install the transmission. Refer to Transmission Replacement . Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 1