For 1990-2009 cars

### Removal Procedure

1. Use a small, flat-bladed tool in order to disengage the sunroof control switch from the headlining module.
2. Disconnect the connector from the sunroof control switch.
3. Remove the sunroof control switch from the vehicle.

### Installation Procedure

1. Connect the connector to the sunroof control switch.
2. Firmly push the sunroof control switch into the headlining module in order to secure the sunroof control switch.