For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Inspect the linkage for improper adjustment or wear. Is there any of these conditions? | Go to Step 2 | Go to Step 3
2 | Repair or replace the linkage as needed. Does the transaxle still slip out of gear? | Go to Step 3 | System OK
3 | Inspect that the transaxle is tight on the engine housing. Is the transaxle loose? | Go to Step 4 | Go to Step 5
4 | Tighten the transaxle to the mounts. Refer to Fastener Tightening Specifications . Does the transaxle still slip out of gear? | Go to Step 5 | System OK
5 | Inspect the shift linkage. Does the shift linkage bind? | Go to Step 6 | Go to Step 7
6 | Repair or replace the shift linkage as needed. Does the transaxle still slip out of gear? | Go to Step 7 | System OK
7 | Inspect the cables. Are they bent or worn? | Go to Step 8 | Go to Step 9
8 | Repair or replace the cables as needed. Does the transaxle still slip out of gear? | Go to Step 9 | System OK
9 | Inspect the input gear bearing retainer . Is the retainer broken or loose? | Go to Step 10 | Go to Step 11
10 | Repair or replace the retainer. Does the transaxle still slip out of gear? | Go to Step 11 | System OK
11 | Inspect the shift fork. Is the shift fork worn or bent? | Go to Step 12 | Go to Step 13
12 | Repair or replace the shift fork as needed. Does the transaxle still slip out of gear? | Go to Step 13 | System OK
13 | Inspect the clutch housing and engine . Is the clutch housing or the engine dirty? | Go to Step 14 | Go to Step 15
14 | Clean the clutch housing and the engine. Does the transaxle still slip out of gear? | Go to Step 15 | System OK
15 | Inspect the shift lever seal. Is the seal stiff? | Go to Step 16 | Go to Step 17
16 | Repair or replace the seal. Does the transaxle still slip out of gear? | Go to Step 17 | System OK
17 | Disassemble the transaxle and repair as necessary. Refer to the M86/M94 Section of the Transmission Unit Repair Manual. Does the transaxle still slip out of gear? | Go to Transmission Replacement | System OK