For 1990-2009 cars

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | Clutch Pedal Position (CPP) Switch
Table 3: | Crankshaft Position (CKP) Sensor
Table 4: | Engine Coolant Temperature (ECT) Sensor
Table 5: | Evaporative Emission (EVAP) Canister Purge Solenoid
Table 6: | Evaporative Emission (EVAP) Canister Vent Solenoid
Table 7: | Fuel Injector 1
Table 8: | Fuel Injector 2
Table 9: | Fuel Injector 3
Table 10: | Fuel Injector 4
Table 11: | Fuel Tank Pressure (FTP) Sensor
Table 12: | Fuel Pump And Sender Assembly
Table 13: | Heated Oxygen Sensor (HO2S) Sensor 2
Table 14: | Idle Air Control (IAC) Valve
Table 15: | Ignition Control Module (ICM)
Table 16: | Intake Air Temperature (IAT) Sensor
Table 17: | Knock Sensor (KS)
Table 18: | Manifold Absolute Pressure (MAP) Sensor
Table 19: | Park/Neutral Position (PNP) Switch, C1
Table 20: | Park/Neutral Position (PNP) Switch, C2
Table 21: | Oxygen Sensor (O2S) Sensor 1
Table 22: | Throttle Position (TP) Sensor
Table 23: | Vehicle Speed Sensor (VSS)

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 633 | CMP Sensor Signal
B | PNK/BLK | 632 | Low Reference
C | RED | 631 | 12 Volt Reference

#### Clutch Pedal Position (CPP) Switch

Connector Part Information |

• | 12034417

• | 2-Way F Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 5 | Crank Voltage
B | PPL | 6 | Stater Solenoid Crank Voltage

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 12162194

• | 2-Way F Metri-Pack 150.2 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 574 | Low Reference
B | YEL | 573 | CKP Sensor (1) Signal

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 2761 | Low Reference
B | YEL | 410 | ECT Sensor Signal

#### Evaporative Emission (EVAP) Canister Purge Solenoid

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Ignition 3 Voltage
B | DK GRN/WHT | 428 | EVAP Canister Purge Solenoid Control

#### Evaporative Emission (EVAP) Canister Vent Solenoid

Connector Part Information |

• | 12059863

• | 2-Way F Metri-Pack 150 Series Sealed (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Ignition 3 Voltage
B | WHT | 1310 | EVAP Canister Vent Solenoid Control

#### Fuel Injector 1

Connector Part Information |

• | 15326179

• | 2-Way F Micro-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 120 | Fuel Pump Supply Voltage
B | BLK | 1744 | Fuel Injector 1 Control

#### Fuel Injector 2

Connector Part Information |

• | 15326179

• | 2-Way F Micro-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 120 | Fuel Pump Supply Voltage
B | LT GRN/BLK | 1745 | Fuel Injector 2 Control

#### Fuel Injector 3

Connector Part Information |

• | 15326179

• | 2-Way F Micro-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 120 | Fuel Pump Supply Voltage
B | PNK/BLK | 1746 | Fuel Injector 3 Control

#### Fuel Injector 4

Connector Part Information |

• | 15326179

• | 2-Way F Micro-Pack 280 Series (BLK)

A | GRY | 120 | Fuel Pump Supply Voltage
B | LT BLU/BLK | 844 | Fuel Injector 4 Control

#### Fuel Tank Pressure (FTP) Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Low Reference
B | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
C | GRY | 416 | 5 Volt Reference

#### Fuel Pump And Sender Assembly

Connector Part Information |

• | 12059110

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 150 | Ground
B | GRY | 120 | Fuel Pump Motor Feed

#### Heated Oxygen Sensor (HO2S) Sensor 2

Connector Part Information |

• | 12160825

• | 4-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1669 | HO2S Low Signal ( - Bank 1 Sensor 2)
B | PPL/WHT | 1668 | HO2S High Signal ( - Bank 1 Sensor 2)
C | BLK | 250 | Ground
D | BRN | 241 | Ignition 3 Voltage

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 12162190

• | 4-Way F Metri-Pack 150.2 Series Pull-to-Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 444 | IAC Coil B Low Control
B | LT GRN/WHT | 1749 | IAC Coil B High Control
C | LT BLU/BLK | 1748 | IAC Coil A Low Control
D | LT BLU/WHT | 1747 | IAC Coil A High Control

#### Ignition Control Module (ICM)

Connector Part Information |

• | 12162838

• | 11-Way F Metri-pack 150.2 Series Pull-to-Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 423 | IC Timing Control
B | ORN | 406 | IC Input 2 - 3
C-E | -- | -- | Not Used
F | YEL | 573 | CKP Sensor (1) Signal
G | PPL/WHT | 430 | Low Resolution Engine Speed Signal
H | RED/BLK | 453 | Low Reference
J | PPL | 574 | Low Reference
K | BLK | 450 | Ground
L | PNK | 239 | Ignition 1 Voltage

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 12162199

• | 2-Way F Metri-Pack 150.2 Series Pull-to-Seat (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2760 | Low Reference
B | TAN | 472 | IAT Sensor Signal

#### Knock Sensor (KS)

Connector Part Information |

• | 12077900

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 496 | KS (1) Signal
B | GRY | 1716 | Reference Low

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | 12129946

• | 3-Way F Metri-Pack 150 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Low Reference
B | LT GRN | 432 | MAP Sensor Signal
C | BRN | 2704 | 5 Volt Reference

#### Park/Neutral Position (PNP) Switch, C1

Connector Part Information |

• | 12129840

• | 7-Way F Metri-Pack Mixed Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | PNK | 539 | Ignition 1 Voltage
C | LT GRN | 275 | Park Neutral Position Switch Park Signal
D | BLK/WHT | 451 | Ground
E | PPL | 6 | Starter Solenoid Crank Voltage
F | LT GRN | 24 | Backup Lamp Supply Voltage
G | YEL | 5 | Crank Voltage

#### Park/Neutral Position (PNP) Switch, C2

Connector Part Information |

• | 12191757

• | 4-Way F Metri-Pack 150 Series Sealed (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 776 | Transmission Range Switch Signal P
B | YEL | 772 | Transmission Range Switch Signal B
C | GRY | 773 | Transmission Range Switch Signal C
D | BLK/WHT | 771 | Transmission Range Switch Signal A

#### Oxygen Sensor (O2S) Sensor 1

Connector Part Information |

• | 15326801

• | 2-Way F Global Terminal 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 413 | HO2S Low Signal
B | PPL | 412 | Pre - Converter O2S 1

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 12110192

• | 3-Way F Metri-Pack 150 Series Pull To Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY/BLK | 2701 | 5 Volt Reference
B | BLK | 2752 | Low Reference
C | DK BLU | 417 | Low Reference

#### Vehicle Speed Sensor (VSS)

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 401 | VSS Low Signal
B | YEL | 400 | VSS High Signal