For 1990-2009 cars

## Refrigerant System Capacities LP1

#### Refrigerant System Capacities

Application | Specification
--- | ---
Metric | English
PAG Oil - GM P/N 12345923 ( Canadian P/N 10953486 )

- Accumulator Replacement

ml*

oz*

* Add 60 ml (2 oz.) of PAG oil plus the equal amount of oil drained from the old accumulator.

- Compressor Replacement

60 ml

2 oz

A Delphi model V-5 compressor is used on RPO (LP1) Only.

- Condenser Replacement

30 ml

1 oz

- Evaporator Replacement

90 ml

3 oz

If more than the specified amount of PAG oil was drained from a component, add the equal amount drained.

- Total System PAG Oil Capacity

266.16 ml

9 oz

- Refrigerant Charge - R134a

0.61 kg

1.35 lb

## Refrigerant System Capacities L61

#### Refrigerant System Capacities

Application | Specification
--- | ---
Metric | English
PAG Oil - GM P/N 12378526 (Canadian P/N 88900060)
Accumulator Replacement | 45 ml* | 1.5 oz*

- * Add PAG oil equal to the amount of oil drained from the old accumulator plus the specified additional amount.

Compressor Replacement | 75 ml¹ | 2.5 oz¹

- A Delphi model CVC-7 compressor is used on the RPO (L61) only.

Condenser Replacement | 30 ml¹ | 1 oz¹
Evaporator Replacement | 60 ml¹ | 2 oz¹

- Total System PAG Oil Capacity

147.0 ml

5 oz

R134a

- Refrigerant Charge

0.61 kg

1.35 lb

¹ If more than the specified amount of PAG oil was drained from a component, add the equal amount drained.