For 1990-2009 cars

Problem | Correction
--- | ---
DEFINITION: The seat is hard to move forward or rearward.
The new adjusters are not broken in. |

- Operate the seat to the full forward or full rearward positions several times in order to work the new tightness out of the channel.

The adjuster(s) are improperly lubricated. |

- Use Lubriplate Auto-Lube in order to lubricate the adjuster channels.

The adjuster(s) are binding due to bent or damaged channels. |

- Replace the adjuster.

The assist springs are disconnected. |

- Reconnect the assist springs.