For 1990-2009 cars

Table 1: | Body Control Module (BCM)
Table 2: | Powertrain Control Module (PCM) 3.4L
Table 3: | Powertrain Control Module (PCM) 2.4L

#### Body Control Module (BCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF
Auto Learn Timer Status | Security Data | Seconds | 0 Seconds
Lockout Timer Status | Security Data | Seconds | 0 Seconds
Passlock Data | Security Data | Invalid/Valid | Valid
Passlock Data Voltage | Security Data | Volts | 3.80 Volts
Passlock Power | Security Data | Active/Inactive | Active
Security Lamp State | Security Data | On/Off | Off
System Type | Security Data | Theft System | Passlock II

#### Powertrain Control Module (PCM) 3.4L

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF
PCM/VCM in VTD Fail Enable | Engine Data 1 | Yes/No | No
VTD Auto Learn Timer | Engine Data 1 | Active/Inactive | Inactive
VTD Fuel Disable | Engine Data 1 | Active/Inactive | Inactive
VTD Fuel Disable Until Ign. OFF | Engine Data 1 | Yes/No | No

#### Powertrain Control Module (PCM) 2.4L

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF
VTD Auto Learn Timer | Engine Data 3 | Active/Inactive | Inactive
VTD Fuel Disable | Engine Data 3 | Active/Inactive | Inactive