For 1990-2009 cars

The radiator support assembly consists of 4 major upper components and 5 major lower components. The following components are preassembled in order to aid in the alignment of the front structure:

• | The center reinforcement

• | The left extensions

• | The right extensions

The upper support is serviced separately in order to provide efficient installation. The lower support is held in place with 6 bolts. The lower support attaches to the 4 brackets that are welded to the lower rails. The brackets are available either as a component of the lower rail service assembly or separately.