For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cooling System

- Engine Cooling, 2.4L

10.7 liters

11.3 quarts

- Engine Cooling, 3.4L

12.9 liters

13.6 quarts

Engine Oil

- With Filter, 2.4L

3.8 liters

4.0 quarts

- With Filter, 3.4L

4.3 liters

4.5 quarts

Fuel Tank | 54.1 liters | 14.3 gallons
Transaxle

- 4T40E/4T45E Transaxle (Bottom Pan Removal)

6.5 liters

6.9 quarts

- 4T40E/4T45E Transaxle (Complete Overhaul)

9.0 liters

9.5 quarts

Manual Transaxle (Complete Drain and Refill) | 1.7 liters | 1.8 quarts
Power Steering System | 0.70 liters | 1.5 pints