For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Bolt | 50 N·m | 37 lb ft
Bypass Pipe Bolt | 21 N·m | 15 lb ft
Camshaft Gear Bolt | 234 N·m | 173 lb ft
Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Camshaft Position Sensor Exciter Ring Bolt | 9 N·m | 80 lb in
Camshaft Thrust Plate Bolt | 22 N·m | 16 lb ft
Connecting Rod Cap Bolt - Angular Tightening Method | 1st Step 64 N·m | 1st Step 47 lb ft
2nd Step 30 degrees | 2nd Step 30 degrees
3rd Step 30 degrees | 3rd Step 30 degrees
Coolant Pipe to Water Pump Nut | 25 N·m | 18 lb ft
Cooling Fan Pulley | 41 N·m | 30 lb ft
Crankshaft Balancer Bolt | 1st Step 100 N·m | 2nd Step 74 lb ft
2nd Step 105 degrees | 2nd Step 105 degrees
Crankshaft Bearing Cap Bolt - Angular Tightening Method | 1st Step 98 N·m | 1st Step 72 lb ft
2nd Step 132 N·m | 2nd Step 97 lb ft
3rd Step 30 degrees | 3rd Step 30 degrees
Crankshaft Bearing Cap Side Bolt | 78 N·m | 58 lb ft
Crankshaft Position Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position Sensor Spacer Bolt | 10 N·m | 89 lb in
Cylinder Head M12 Bolt - Angular Tightening Method | 1st Step 50 N·m | 1st Step 37 lb ft
2nd Step 80 N·m | 2nd Step 59 lb ft
3rd Step 60 degrees
4th Step 60 degrees
Cylinder Head M8 Bolt | 25 N·m | 18 lb ft
Drive Belt Tensioner Pulley Bolt | 41 N·m | 30 lb ft
Engine Block Coolant Plug | 18 N·m | 13 lb ft
Engine Block Ground Bolt | 34 N·m | 25 lb ft
Engine Mount to Block Bolts | 58 N·m | 43 lb ft
Exhaust Manifold Bolt/Nut | 38 N·m | 28 lb ft
Exhaust Manifold Heat Shield Bolts | 8 N·m | 71 lb in
Exhaust Outlet Clamp | 15 N·m | 11 lb ft
Exhaust Outlet Heat Shield Bolts | 8 N·m | 71 lb in
Exhaust Outlet Pipe Bolt | 53 N·m | 39 lb ft
Exhaust Pipe Bolt | 53 N·m | 39 lb ft
Exhaust Pipe Bracket Bolt | 34 N·m | 25 lb ft
Exhaust Pipe Heat Shield Bolts | 8 N·m | 71 lb in
Fan Pulley Bracket Bolt | 46 N·m | 34 lb ft
Flywheel Bolt - Angular Tightening Method | 1st Step 79 N·m | 1st Step 58 lb ft
2nd Step 60 degrees | 2nd Step 60 degrees
3rd Step 60 degrees | 3rd Step 60 degrees
Flywheel Housing Bolt - Black Circle Mark | 90 N·m | 67 lb ft
Flywheel Housing to Upper Oil Pan Bolt - Black Triangle Mark | 50 N·m | 37 lb ft
Front Engine Cover Bolt | 21 N·m | 15 lb ft
Fuel Block Bolt | 25 N·m | 18 lb ft
Fuel Filter Bracket Bolt | 21 N·m | 15 lb ft
Fuel Injection Control Module Bolt | 20 N·m | 15 lb ft
Fuel Injection Control Module Bracket Bolt | 21 N·m | 15 lb ft
Fuel Injection Control Module Connector Bolt | 10 N·m | 89 lb in
Fuel Injection Control Module Connector Bracket Bolt | 21 N·m | 15 lb ft
Fuel Injection Control Module Cooler Eye Bolt | 27 N·m | 20 lb ft
Fuel Injection Pipe Nut | 41 N·m | 30 lb ft
Fuel Inlet Pipe Bracket Bolt | 21 N·m | 15 lb ft
Fuel Pipes Bracket Bolt | 25 N·m | 18 lb ft
Fuel Rail Assembly Bolt | 25 N·m | 18 lb ft
Fuel Rail Connector | 45 N·m | 33 lb ft
Fuel Return Pipe Eye Bolt - Cylinder Head Side | 17 N·m | 12 lb ft
Fuel Return Pipe Eye Bolt - Injector Side | 16 N·m | 12 lb ft
Fuel Return Pipe Sleeve Nut | 41 N·m | 30 lb ft
Fuel Return Sleeve Unit | 41 N·m | 30 lb ft
Fuel Injection Pump Assembly to Cylinder Block Bolt | 21 N·m | 15 lb ft
Fuel Injection Pump to Bracket Bolt | 21 N·m | 15 lb ft
Fuel Injection Pump Drive Gear Nut | 70 N·m | 52 lb ft
Fuel Temperature Sensor Eye Bolt | 15 N·m | 11 lb ft
Function Block Nut | 25 N·m | 18 lb ft
Function Block to Injection Pipe Nut | 41 N·m | 30 lb ft
Generator Bracket Bolt | 50 N·m | 37 lb ft
Glow Plug | 18 N·m | 13 lb ft
Glow Plug Connector Nut | 2 N·m | 18 lb in
Glow Plug Power Feed Nut | 15 N·m | 11 lb ft
Glow Plug Relay Assembly Bolt | 25 N·m | 18 lb ft
Heater Pipe Bolt | 21 N·m | 15 lb ft
Idle Pulley Bolt/Screw | 37 N·m | 27 lb ft
Injector Bracket Bolt | 50 N·m | 37 lb ft
Injector Harness Bracket Bolt | 9 N·m | 80 lb in
Injector Terminal Nut | 2 N·m | 18 lb in
Injector Pipe Lock Plate Screws | 4 N·m | 35 lb in
Intake Air Heater | 50 N·m | 37 lb ft
Intake Manifold Bolts/Nuts | 21 N·m | 15 lb ft
Intake Manifold Tube Bolts/Nuts | 9 N·m | 80 lb in
Oil Cooler Adapter Bolts | 21 N·m | 15 lb ft
Oil Cooler Adapter Nuts | 25 N·m | 18 lb ft
Oil Cooler Assembly Bolts | 25 N·m | 18 lb ft
Oil Cooler Adapter Stud | 10 N·m | 89 lb in
Oil Drain Plug | 84 N·m | 62 lb ft
Oil Fill Tube Bolt | 21 N·m | 15 lb ft
Oil Filter | 21 N·m | 15 lb ft
Oil Gallery Plugs | 53 N·m | 39 lb ft
Oil Level Indicator Tube Bolt | 21 N·m | 15 lb ft
Oil Level Sensor Bolt | 10 N·m | 89 lb in
Oil Pan Bolts/Nuts - Lower | 10 N·m | 89 lb in
Oil Pan Bolt - Upper | 20 N·m | 15 lb ft
Oil Pressure Sensor Adapter Eye Bolt | 38 N·m | 28 lb ft
Oil Pressure Sensor Unit | 30 N·m | 22 lb ft
Oil Pressure Relief Valve | 39 N·m | 29 lb ft
Oil Pump Bolt | 21 N·m | 15 lb ft
Oil Pump Driven Gear Nut | 100 N·m | 74 lb ft
Oil Pump Gear Cover Bolt | 21 N·m | 15 lb ft
Oil Strainer Bolts/Nuts | 25 N·m | 18 lb ft
Piston Cooling Nozzle Eye Bolt | 21 N·m | 15 lb ft
Positive Crankcase Ventilation Cover Screws | 4 N·m | 35 lb in
Power Steering Pump Bolt | 50 N·m | 37 lb ft
Power Steering Pump Bracket Bolt | 46 N·m | 34 lb ft
Rocker Arm Shaft Bracket Bolt | 41 N·m | 30 lb ft
Starter Motor Bolt | 78 N·m | 58 lb ft
Thermostat Housing Bolts/Nuts | 25 N·m | 18 lb ft
Thermostat Cover Bolt | 21 N·m | 15 lb ft
Turbocharger Bolt | 108 N·m | 80 lb ft
Turbocharger Boost Sensor Bolt | 10 N·m | 89 lb in
Turbocharger Coolant Outlet Pipe Bracket Bolts | 21 N·m | 15 lb ft
Turbocharger Heat Shield Bolts | 9 N·m | 80 lb in
Turbocharger Inlet Duct to Turbocharger Bolt | 9 N·m | 80 lb in
Turbocharger Oil Return Pipe Stud | 10 N·m | 89 lb in
Turbocharger Oil Supply Hose Eye Bolt | 34 N·m | 25 lb ft
Turbocharger Oil Return Pipe Bolts/Nuts | 21 N·m | 15 lb ft
Turbocharger Thermostatic Coolant Valve | 60 N·m | 44 lb ft
Upper Oil Pan to Flywheel Housing Screws | 20 N·m | 15 lb ft
Valve Adjusting Screw Nut | 22 N·m | 16 lb ft
Valve Lifter Holdown Bracket Bolt | 11 N·m | 97 lb in
Valve Rocker Arm Cover Bolt - Lower | 10 N·m | 89 lb in
Valve Rocker Arm Cover Bolt - Upper | 8 N·m (Two Times) | 71 lb in (Two Times)
Water Outlet Bolts | 25 N·m | 18 lb ft
Water Pump Bolt | 21 N·m | 15 lb ft