QUARTER WINDOW GLASS LOOSE REPLACE SWING OUT GLASS. Oldsmobile Custom Cruiser 1991

For 1990-2009 cars

# QUARTER WINDOW GLASS LOOSE REPLACE SWING OUT GLASS

#### SUBJECT: SWING OUT QUARTER WINDOW GLASS LOOSE AT HINGES - REPLACE SWING OUT GLASS

#### MODELS/YEARS: 1991-92 CUSTOM CRUISER

#### CONDITION:

---------- A condition may exist where the swing out quarter window glass may become loose at the hinge area.

#### CAUSE:

------ Hinge bond material releases.

#### CORRECTION:

----------- Replace the swing out glass only, using the following part numbers and the procedure found in the Service Manual, Section 10-7. Parts are currently available from GMSPO.

12506798 Right Side 12506797 Left Side

#### IMPORTANT: ---------- 1. Do not attempt to reglue the hinge to the glass.

2. Do not replace the complete quarter glass module to make this repair.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.