INOPERATIVE 3RD SEAT RELEASE- NEW AND IMPROVED REPAIR PARTS. Oldsmobile Custom Cruiser 1986

For 1990-2009 cars

# INOPERATIVE 3RD SEAT RELEASE- NEW AND IMPROVED REPAIR PARTS

R MODELS/YEARS: 1977-86 CUSTOM CRUISER WAGONS

Some 1977 through 1986 Custom Cruiser wagons are being returned to dealers because of an inoperative 3rd seat back release system.

This condition may be caused by the seat back release cable becoming disengaged from the release handle or the release handle breaking because of high operating efforts.

When repairing vehicies with this condition, new improved parts are available from WDDGM. The new parts that make up the seat back release system cannot be used with parts from the original system. Therefore, when repair is required, parts from the original system must be completely replaced with new parts. To determine if a system is of the new type, inspect the end of the cable assembly that attaches to the new release handle. A cable that is part of the new system will have an opening that engages the release handle. See Figure 1.

If the vehicle is within the basic 12/12 warranty coverage period, submit a warranty claim using the labor operation number and time listed in the Oldsmobile Labor Time Guide for the appropriate year of the vehicle.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.