ENGINE WIRE HARNESS MAY BE DAMAGED BY ENGINE BLOCK. Oldsmobile Custom Cruiser 1992

For 1990-2009 cars

# ENGINE WIRE HARNESS MAY BE DAMAGED BY ENGINE BLOCK

#### SUBJECT: ENGINE WIRE HARNESS MAY BE DAMAGED BY ENGINE BLOCK (REPOSITION AND SECURE HARNESS)

#### VEHICLES AFFECTED: 1991-92 B-CAR

#### Note: Only the Buick Sedan is a 1992 Model.

#### Condition:

---------- The main electrical harness (right rear side of engine) may contact the engine (see illustration). The heat from the engine block may damage the harness by shorting the wires to the block.

#### Cause:

------ The harness may be pushed forward from it's normal position, allowing contact with the engine block. A clip was added in production after the following VIN'S:

Assembly Plant Division VIN -------------- ---------- -------- Arlington Buick (92) NR402868 Chevrolet MR129841

Willow Run Chevrolet MW240159 Buick wagon MW403073 Olds Wagon MW305367

#### Correction:

----------- 1. Disconnect negative battery cable.

2. Raise vehicle. Remove right front wheel and tire. Remove inner fender splash shield.

3. Inspect harness, and repair any damage as necessary.

4. Remove the plastic push-in clip from the bracket. The push-in clip can be left on the harness to locate the new clip.

5. Use clip, P/N 12010517, and self-tapping screw, P/N 11500086, to retain the harness to the bracket as shown in the illustration. Straighten bracket if necessary. Make sure the clip stays vertical after the screw is tightened.

6. Install inner fender splash shield. Install wheel and tire. Lower vehicle.

7. Reconnect negative battery cable.

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.