RUST FORMING ON LUGGAGE RACK SCREWS REPLACE SLATS & SCREWS. Oldsmobile Custom Cruiser 1991

For 1990-2009 cars

# RUST FORMING ON LUGGAGE RACK SCREWS REPLACE SLATS & SCREWS

#### SUBJECT: RUST FORMING ON LUGGAGE RACK SLAT SCREWS (REPLACE SLATS AND SCREWS)

#### VEHICLES AFFECTED: 1991 B CAR

Condition: Rust forming on luggage rack slat screws.

Cause: Galvanic corrosion between screw and metal reinforcement in slat.

Correction: Replace slats and screws with the following part numbers as outlined in the service manual.

Chevrolet slat part number: 10196178 (5 required)

Chevrolet screw part number: 10196105 (25 required)

Buick and Oldsmobile slat part number: 10196179 - (5 required) Buick and Oldsmobile screw part number: 10196105 - (20 required)

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.